Contents of IBIS_AMI_Tx.ami as read by ami2csv

IBIS_AMI_Tx
    Description     Generic transmitter model published by SiSoft
    Reserved_Parameters
        Ignore_Bits
            Usage       Info
            Type        Integer
            Default     4
            Description     Ignore four bits to fill up tapped delay line.
        Max_Init_Aggressors
            Usage       Info
            Type        Integer
            Default     25
            Description     Number of aggressors is actually unlimited.
        Init_Returns_Impulse
            Usage       Info
            Type        Boolean
            Default     True
            Description     Both impulse and parameters_out returned.
        GetWave_Exists
            Usage       Info
            Type        Boolean
            Default     True
            Description     GetWave is well and truly provided in the module.
    Model_Specific
        tap_filter
            Description     Array of transmit de-emphasis tap weights
            -1
                Usage       InOut
                Range       0.0 -1.0    1.0
                Type        Tap
                Default     0
                Description     Pre-cursor tap weight
            0
                Usage       InOut
                Range       1.0 -1.0    1.0
                Type        Tap
                Default     1
                Description     Main tap weight
            1
                Usage       InOut
                Range       0.0 -1.0    1.0
                Type        Tap
                Default     0
                Description     First post-cursor tap weight
            2
                Usage       InOut
                Range       0.0 -1.0    1.0
                Type        Tap
                Default     0
                Description     Second post-cursor tap weight
        tx_swing
            Usage       In
            Range       0.8 0.3 1.0
            Type        Float
            Default     0.8
            Description     Peak differential output voltage
