# Instantiated Subckts

The instantiated subckts appear in the lower section. Change the node names to establish the test circuit netlist.

Previous slide | Next slide | Back to first slide | View graphic version

Notes:

Set the node name by triple clicking before you type. The names are:

pad input ena vdd vss

rcvrout pad vdd vss

After entering the last name, be sure to click on some other cell, to

have the last entry taken.